*Heading
** billet_case1_std_coarse_cax4i.inp
** ABAQUS/Standard:  Case 1
**
** PARTS
**
*Part, name=Billet
*End Part
*Part, name=RIGID
*End Part
**
** ASSEMBLY
**
*Assembly, name=Assembly
**
*Instance, name=Billet-1, part=Billet
*Node, input=billet_coarse_nodes.inp
*Element, type=CAX4I, input=billet_coarse_elem.inp
** Region: (BILLET:Picked)
*Elset, elset=_I1, internal, generate
** Section: BILLET
*Solid Section, elset=_I1, material=METAL
1.,
*End Instance
**
*Instance, name=RIGID-1, part=RIGID
*Node
*Nset, nset=RIGID-1-RefPt_, internal
*Surface, type=SEGMENTS, name=RIGID
START,         0.02,        0.015
 LINE,           0.,        0.015
*Rigid Body, ref node=RIGID-1-RefPt_, analytical surface=RIGID
*End Instance
*Nset, nset=NRIGID, instance=RIGID-1
*Nset, nset=MIDDLE, instance=Billet-1, generate
*Elset, elset=MIDDLE, instance=Billet-1, generate
*Nset, nset=AXIS, instance=Billet-1, generate
*Elset, elset=AXIS, instance=Billet-1, generate
*Elset, elset=_ASURF_S2, internal, instance=Billet-1, generate
*Elset, elset=_ASURF_S3, internal, instance=Billet-1, generate
*Surface, type=ELEMENT, name=ASURF
_ASURF_S2, S2
_ASURF_S3, S3
*End Assembly
**
** MATERIALS
**
*Material, name=METAL
*Elastic
 2e+11, 0.3
*Plastic
   7e+08, 0.
 3.7e+09,10.
**
** INTERACTION PROPERTIES
**
*Surface Interaction, name=ROUGH
1.,
*Friction, rough
*Surface Behavior, pressure-overclosure=HARD
**
** BOUNDARY CONDITIONS
**
** Name: AXIS Type: Displacement/Rotation
*Boundary
AXIS, 1, 1
** Name: FIX_RIGID Type: Displacement/Rotation
*Boundary
NRIGID, 1, 1
NRIGID, 6, 6
** Name: MIDDLE Type: Displacement/Rotation
*Boundary
MIDDLE, 2, 2
**
** INTERACTIONS
**
** Interaction: RIGID to ASURF
*Contact Pair, interaction=ROUGH
ASURF, RIGID-1.RIGID
** ----------------------------------------------------------------
**
** STEP: STEP-1
**
*Step, nlgeom, inc=200
STEP-1: 73.3 PERCENT OF DIE DISPLACEMENT
 (44% BILLET UPSET)
*Static
0.015, 1., 1e-05, 1.
**
** BOUNDARY CONDITIONS
**
** Name: RIGID_44_PERCENT Type: Displacement/Rotation
*Boundary
NRIGID, 2, 2, -0.0066
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=1
*Monitor, dof=2, node=NRIGID, frequency=2
*Output, field, variable=PRESELECT
*Output, history, frequency=1
*Energy Output
ALLAE, ALLCD, ALLFD, ALLIE, ALLKE, ALLPD, ALLSE, ALLVD, ALLWK, ETOTAL
*Output, history, frequency=1
*Node Output, nset=NRIGID
U2, RF2
*El Print, freq=999999
*Node Print, freq=999999
*Contact File, slave=ASURF, frequency=40
*Node File, nset=NRIGID
U,RF
*End Step
** ----------------------------------------------------------------
**
** STEP: STEP-2
**
*Step, inc=200
STEP-2: 100 PERCENT OF DIE DISPLACEMENT
 (60% BILLET UPSET)
*Static
0.015, 1., 1e-05, 1.
**
** BOUNDARY CONDITIONS
**
** Name: RIGID_44_PERCENT Type: Displacement/Rotation
*Boundary
NRIGID, 2, 2, -0.009
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=1
*Output, field, variable=PRESELECT
*Output, history, frequency=1
*Energy Output
ALLAE, ALLCD, ALLFD, ALLIE, ALLKE, ALLPD, ALLSE, ALLVD, ALLWK, ETOTAL
*Output, history, frequency=1
*Node Output, nset=NRIGID
U2, RF2
*Contact File, slave=ASURF, frequency=40
*Node File, nset=NRIGID
U,RF
*End Step