*Heading
** Job name: controlArm Model name: controlArm
**
** PARTS
**
*Part, name=PART-1
*Node
*Element, type=C3D10
*Elset, elset=All_Solid_Elements
*End Part
**
**
** ASSEMBLY
**
*Assembly, name=Assembly
**
*Instance, name=PART-1-1, part=PART-1
*End Instance
**
*Nset, nset=CONTROLPT, instance=PART-1-1
*Nset, nset=CONSTR1_SURF, instance=PART-1-1
*Nset, nset=CONSTR2_SURF, instance=PART-1-1, generate
*Nset, nset=PINNED_NODES, instance=PART-1-1
*Nset, nset=SYMMETRY_PLANE, instance=PART-1-1
*Nset, nset=LEFT_FIXTURE, instance=PART-1-1
*Elset, elset=DESIGN_ELEMENTS, instance=PART-1-1
*Elset, elset=_PICKEDSET11, internal, instance=PART-1-1
*Elset, elset=FROZEN_AREA, instance=PART-1-1
*End Assembly
**
** BOUNDARY CONDITIONS
**
** Name: Disp-BC-1 Type: Displacement/Rotation
*Boundary
CONTROLPT, 3, 3
** Name: Disp-BC-2 Type: Symmetry/Antisymmetry/Encastre
*Boundary
PINNED_NODES, PINNED
** ----------------------------------------------------------------
**
** STEP: Step-1
**
*Step, name=Step-1, perturbation
SUBTITLE=LASTFALL1
*Static
**
** BOUNDARY CONDITIONS
**
** Name: Disp-BC-3 Type: Displacement/Rotation
*Boundary
SYMMETRY_PLANE, 3, 3
** Name: Disp-BC-4 Type: Displacement/Rotation
*Boundary
LEFT_FIXTURE, 1, 3
**
** OUTPUT REQUESTS
**
**
** FIELD OUTPUT: F-Output-1
**
*Output, field, variable=PRESELECT
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step