*HEADING
 EXPLOSIVELY LOADED CYLINDRICAL PANEL: 128 x 256 mesh
**
*RESTART,WRITE,NUMBER INTERVAL=5,TIMEMARKS=NO
*PREPRINT,ECHO=NO,MODEL=NO,HISTORY=NO
**
*NODE
**
*NGEN,NSET=EDGEA,LINE=C
*NGEN,NSET=EDGEB,LINE=C
*NFILL
 EDGEA,EDGEB,256,129
*NSET,NSET=EDGEC,GENERATE
*NSET,NSET=EDGED,GENERATE
*ELEMENT,TYPE=S4R
*ELGEN,ELSET=SHELL
*BOUNDARY
 EDGEA,ENCASTRE
 EDGEB,ENCASTRE
 EDGEC,ENCASTRE
 EDGED,XSYMM
*SHELL SECTION,ELSET=SHELL,MATERIAL=ALUMINUM
 0.125,
**
*MATERIAL,NAME=ALUMINUM
*ELASTIC
 10.5E6, 0.333
*PLASTIC
 4.4E4,
*DENSITY
 2.5E-4,
**
*NSET,NSET=BLAST1,GENERATE
*NSET,NSET=BLAST2,GENERATE
*NSET,NSET=BLAST3,GENERATE
*NSET,NSET=BLAST4,GENERATE
*NSET,NSET=BLAST5,GENERATE
*NSET,NSET=BLAST6,GENERATE
*NSET,NSET=BLAST7,GENERATE
*NSET,NSET=BLAST8,GENERATE
*NSET,NSET=BLAST9,GENERATE
*NSET,NSET=BLAST10,GENERATE
*NSET,NSET=BLAST11,GENERATE
*NSET,NSET=BLAST12,GENERATE
*NSET,NSET=BLAST13,GENERATE
*NSET,NSET=BLAST14,GENERATE
*NSET,NSET=BLAST15,GENERATE
*NSET,NSET=BLAST16,GENERATE
*NSET,NSET=BLAST17,GENERATE
*NSET,NSET=BLAST18,GENERATE
*NSET,NSET=BLAST19,GENERATE
*NSET,NSET=BLAST20,GENERATE
*NSET,NSET=BLAST21,GENERATE
*NSET,NSET=BLAST22,GENERATE
*NSET,NSET=BLAST23,GENERATE
*NSET,NSET=BLAST24,GENERATE
*NSET,NSET=BLAST25,GENERATE
*NSET,NSET=BLAST26,GENERATE
*NSET,NSET=BLAST27,GENERATE
*NSET,NSET=BLAST28,GENERATE
*NSET,NSET=BLAST29,GENERATE
*NSET,NSET=BLAST30,GENERATE
*NSET,NSET=BLAST31,GENERATE
*NSET,NSET=BLAST32,GENERATE
*NSET,NSET=BLAST33,GENERATE
*NSET,NSET=BLAST34,GENERATE
*NSET,NSET=BLAST35,GENERATE
*NSET,NSET=BLAST36,GENERATE
*NSET,NSET=BLAST37,GENERATE
*NSET,NSET=BLAST38,GENERATE
*NSET,NSET=BLAST39,GENERATE
*NSET,NSET=BLAST40,GENERATE
*NSET,NSET=BLAST41,GENERATE
*NSET,NSET=BLAST42,GENERATE
*NSET,NSET=BLAST43,GENERATE
*NSET,NSET=BLAST44,GENERATE
*NSET,NSET=BLAST45,GENERATE
*NSET,NSET=BLAST46,GENERATE
*NSET,NSET=BLAST47,GENERATE
*NSET,NSET=BLAST48,GENERATE
*NSET,NSET=BLAST49,GENERATE
*NSET,NSET=BLAST50,GENERATE
*NSET,NSET=BLAST51,GENERATE
*NSET,NSET=BLAST52,GENERATE
*NSET,NSET=BLAST53,GENERATE
*NSET,NSET=BLAST54,GENERATE
*NSET,NSET=BLAST55,GENERATE
*NSET,NSET=BLAST56,GENERATE
*NSET,NSET=BLAST57,GENERATE
*NSET,NSET=BLAST58,GENERATE
*NSET,NSET=BLAST59,GENERATE
*NSET,NSET=BLAST60,GENERATE
*NSET,NSET=BLAST61,GENERATE
*NSET,NSET=BLAST62,GENERATE
*NSET,NSET=BLAST63,GENERATE
*NSET,NSET=BLAST64,GENERATE
*NSET,NSET=BLAST65,GENERATE
**
*INITIAL CONDITIONS,TYPE=VELOCITY
 BLAST1, 3, -5650.0
 BLAST2, 3, -5649.8
 BLAST3, 3, -5649.2
 BLAST4, 3, -5648.3
 BLAST5, 3, -5647.0
 BLAST6, 3, -5645.3
 BLAST7, 3, -5643.2
 BLAST8, 3, -5640.7
 BLAST9, 3, -5637.9
 BLAST10, 3, -5634.7
 BLAST11, 3, -5631.1
 BLAST12, 3, -5627.1
 BLAST13, 3, -5622.8
 BLAST14, 3, -5618.1
 BLAST15, 3, -5613.0
 BLAST16, 3, -5607.5
 BLAST17, 3, -5601.7
 BLAST18, 3, -5595.4
 BLAST19, 3, -5588.8
 BLAST20, 3, -5581.9
 BLAST21, 3, -5574.5
 BLAST22, 3, -5566.8
 BLAST23, 3, -5558.7
 BLAST24, 3, -5550.3
 BLAST25, 3, -5541.4
 BLAST26, 3, -5532.2
 BLAST27, 3, -5522.7
 BLAST28, 3, -5512.7
 BLAST29, 3, -5502.4
 BLAST30, 3, -5491.7
 BLAST31, 3, -5480.7
 BLAST32, 3, -5469.3
 BLAST33, 3, -5457.5
 BLAST34, 3, -5445.3
 BLAST35, 3, -5432.8
 BLAST36, 3, -5419.9
 BLAST37, 3, -5406.7
 BLAST38, 3, -5393.1
 BLAST39, 3, -5379.2
 BLAST40, 3, -5364.8
 BLAST41, 3, -5350.2
 BLAST42, 3, -5335.1
 BLAST43, 3, -5319.7
 BLAST44, 3, -5304.0
 BLAST45, 3, -5287.9
 BLAST46, 3, -5271.4
 BLAST47, 3, -5254.6
 BLAST48, 3, -5237.4
 BLAST49, 3, -5219.9
 BLAST50, 3, -5202.1
 BLAST51, 3, -5183.8
 BLAST52, 3, -5165.3
 BLAST53, 3, -5146.4
 BLAST54, 3, -5127.1
 BLAST55, 3, -5107.5
 BLAST56, 3, -5087.6
 BLAST57, 3, -5067.3
 BLAST58, 3, -5046.7
 BLAST59, 3, -5025.8
 BLAST60, 3, -5004.5
 BLAST61, 3, -4982.9
 BLAST62, 3, -4960.9
 BLAST63, 3, -4938.6
 BLAST64, 3, -4916.0
 BLAST65, 3, -4893.0
**
 BLAST1, 1,     0.0
 BLAST2, 1,   -46.2
 BLAST3, 1,   -92.4
 BLAST4, 1,  -138.7
 BLAST5, 1,  -184.9
 BLAST6, 1,  -231.1
 BLAST7, 1,  -277.2
 BLAST8, 1,  -323.4
 BLAST9, 1,  -369.5
 BLAST10, 1,  -415.6
 BLAST11, 1,  -461.7
 BLAST12, 1,  -507.8
 BLAST13, 1,  -553.8
 BLAST14, 1,  -599.8
 BLAST15, 1,  -645.7
 BLAST16, 1,  -691.6
 BLAST17, 1,  -737.5
 BLAST18, 1,  -783.3
 BLAST19, 1,  -829.0
 BLAST20, 1,  -874.7
 BLAST21, 1,  -920.4
 BLAST22, 1,  -965.9
 BLAST23, 1, -1011.4
 BLAST24, 1, -1056.9
 BLAST25, 1, -1102.3
 BLAST26, 1, -1147.6
 BLAST27, 1, -1192.8
 BLAST28, 1, -1237.9
 BLAST29, 1, -1283.0
 BLAST30, 1, -1328.0
 BLAST31, 1, -1372.8
 BLAST32, 1, -1417.6
 BLAST33, 1, -1462.3
 BLAST34, 1, -1506.9
 BLAST35, 1, -1551.4
 BLAST36, 1, -1595.8
 BLAST37, 1, -1640.1
 BLAST38, 1, -1684.3
 BLAST39, 1, -1728.4
 BLAST40, 1, -1772.3
 BLAST41, 1, -1816.1
 BLAST42, 1, -1859.8
 BLAST43, 1, -1903.4
 BLAST44, 1, -1946.9
 BLAST45, 1, -1990.2
 BLAST46, 1, -2033.4
 BLAST47, 1, -2076.5
 BLAST48, 1, -2119.4
 BLAST49, 1, -2162.2
 BLAST50, 1, -2204.8
 BLAST51, 1, -2247.3
 BLAST52, 1, -2289.6
 BLAST53, 1, -2331.8
 BLAST54, 1, -2373.8
 BLAST55, 1, -2415.7
 BLAST56, 1, -2457.4
 BLAST57, 1, -2498.9
 BLAST58, 1, -2540.3
 BLAST59, 1, -2581.5
 BLAST60, 1, -2622.5
 BLAST61, 1, -2663.4
 BLAST62, 1, -2704.1
 BLAST63, 1, -2744.6
 BLAST64, 1, -2784.9
 BLAST65, 1, -2825.0
**
** The following three elements in elset QA_TEST are
** equally spaced along the edge D.
**
*ELSET,ELSET=QA_TEST
*NSET,NSET=QA_TEST
**
** Run the problem for 1 milliseconds
**
*STEP
*DYNAMIC,EXPLICIT
 ,1.E-3
*MONITOR,NODE=16513,DOF=3
*OUTPUT,FIELD,VAR=PRESELECT,NUMBER INTERVAL=5
**
** Output requests for qa testing
**
*OUTPUT,FIELD,NUMBER INTERVAL=4,TIMEMARKS=YES
*ELEMENT OUTPUT, ELSET=QA_TEST
 PEEQ,
*NODE OUTPUT, NSET=QA_TEST
 U,
*OUTPUT,HISTORY,VAR=PRESELECT,TIME INTERVAL=2.5E-4
*FILE OUTPUT,NUM=4,TIMEMARKS=YES
*EL FILE,ELSET=QA_TEST
 PEEQ,
*NODE FILE,NSET=QA_TEST
 U,
*ENERGY FILE
**
***OUTPUT,HISTORY,TIME INTERVAL=0.0
***ELEMENT OUTPUT,ELSET=ELOUT
**SF,STH
***ELEMENT OUTPUT,ELSET=ELOUT,SECTIONPOINT=1
**PEEQ,MISES
***ELEMENT OUTPUT,ELSET=ELOUT,SECTIONPOINT=2
**PEEQ,MISES
***ELEMENT OUTPUT,ELSET=ELOUT,SECTIONPOINT=3
**PEEQ,MISES
***NODE OUTPUT,NSET=A
**U,V
***ENERGY OUTPUT
**ALLKE,ALLIE,ALLSE,ALLAE,ALLVD,ALLCD,ALLPD,ALLFD,ALLWK,ETOTAL,DT
*END STEP