*HEADING
 EXPLOSIVELY LOADED CYLINDRICAL PANEL: 32 x 64 mesh
**
*RESTART,WRITE,NUMBER INTERVAL=5,TIMEMARKS=NO
*PREPRINT,ECHO=NO,MODEL=NO,HISTORY=NO
**
*NODE
*NGEN,NSET=EDGEA,LINE=C
*NGEN,NSET=EDGEB,LINE=C
*NFILL
EDGEA,EDGEB,64,100
*NSET,NSET=EDGEC,GENERATE
*NSET,NSET=EDGED,GENERATE
*ELEMENT,TYPE=S4RSW
*ELGEN,ELSET=SHELL
*BOUNDARY
EDGEA,ENCASTRE
EDGEB,ENCASTRE
EDGEC,ENCASTRE
EDGED,XSYMM
*SHELL SECTION,ELSET=SHELL,MATERIAL=ALUMINUM,SECTION INTE=GAUSS,OFFSET=0.5
.125,
**
*MATERIAL,NAME=ALUMINUM
*ELASTIC
10.5E6,0.333
*PLASTIC
4.4E4,
*DENSITY
2.5E-4,
**
*NSET,NSET=BLAST1,GENERATE
*NSET,NSET=BLAST2,GENERATE
*NSET,NSET=BLAST3,GENERATE
*NSET,NSET=BLAST4,GENERATE
*NSET,NSET=BLAST5,GENERATE
*NSET,NSET=BLAST6,GENERATE
*NSET,NSET=BLAST7,GENERATE
*NSET,NSET=BLAST8,GENERATE
*NSET,NSET=BLAST9,GENERATE
*NSET,NSET=BLAST10,GENERATE
*NSET,NSET=BLAST11,GENERATE
*NSET,NSET=BLAST12,GENERATE
*NSET,NSET=BLAST13,GENERATE
*NSET,NSET=BLAST14,GENERATE
*NSET,NSET=BLAST15,GENERATE
*NSET,NSET=BLAST16,GENERATE
*NSET,NSET=BLAST17,GENERATE
*INITIAL CONDITIONS,TYPE=VELOCITY
BLAST1, 3,-5650.
BLAST2, 3,-5647.
BLAST3, 3,-5638.
BLAST4, 3,-5602.
BLAST5, 3,-5575.
BLAST6, 3,-5541.
BLAST7, 3,-5502.
BLAST8, 3,-5457.
BLAST9, 3,-5407.
BLAST10,3,-5350.
BLAST11,3,-5288.
BLAST12,3,-5220.
BLAST13,3,-5146.
BLAST14,3,-5067.
BLAST15,3,-5983.
BLAST16,3,-4993.
BLAST17,3,-4893.
BLAST1, 1,-0.
BLAST2, 1,-185.
BLAST3, 1,-370.
BLAST4, 1,-554.
BLAST5, 1,-737.
BLAST6, 1,-920.
BLAST7, 1,-1102.
BLAST8, 1,-1283.
BLAST9, 1,-1463.
BLAST10,1,-1640.
BLAST11,1,-1816.
BLAST12,1,-1990.
BLAST13,1,-2162.
BLAST14,1,-2332.
BLAST15,1,-2499.
BLAST16,1,-2663.
BLAST17,1,-2825.
**
*ELSET, ELSET=ELOUT
*NSET,NSET=A
*ELSET,ELSET=QA_TEST_ELOUT
ELOUT,
*NSET,NSET=QA_TEST_A
A,
**
*STEP
*DYNAMIC,EXPLICIT
,1.E-3
*BULK VISCOSITY
*MONITOR,NODE=3201,DOF=3
*FILE OUTPUT,NUM=4,TIMEMARKS=YES
*EL FILE, ELSET=ELOUT
 PEEQ,
*NODE FILE, NSET=A
 U,
*ENERGY FILE
***OUTPUT,HISTORY,TIME INTERVAL=0.0
***ENERGY OUTPUT
**ALLAE,ALLIE,ALLKE,ALLPD,ALLSE,ALLVD,ALLWK,ETOTAL
***ELEMENT OUTPUT,ELSET=ELOUT
**SF,STH
***ELEMENT OUTPUT,ELSET=ELOUT,SECTIONPOINT=1
**PEEQ,MISES
***ELEMENT OUTPUT,ELSET=ELOUT,SECTIONPOINT=2
**PEEQ,MISES
***ELEMENT OUTPUT,ELSET=ELOUT,SECTIONPOINT=3
**PEEQ,MISES
***NODE OUTPUT,NSET=A
**U,V
*OUTPUT, FIELD, NUMBER INTERVAL=4, TIMEMARKS=YES
*ELEMENT OUTPUT, ELSET=QA_TEST_ELOUT
 PEEQ,
*NODE OUTPUT, NSET=QA_TEST_A
 U,
*OUTPUT,FIELD,VARIABLE=PRESELECT
*OUTPUT,HISTORY,VARIABLE=PRESELECT,TIMEINT=0.00025
*END STEP