*HEADING
 EXPLOSIVELY LOADED CYLINDRICAL PANEL: 8 x 32 mesh
**
*RESTART,WRITE,NUMBER INTERVAL=5,TIMEMARKS=NO
*PREPRINT,ECHO=NO,MODEL=NO,HISTORY=NO
**
*NODE
*NGEN,NSET=EDGEA,LINE=C
*NGEN,NSET=EDGEB,LINE=C
*NFILL
EDGEA,EDGEB,64,100
*NSET,NSET=EDGEC,GENERATE
*NSET,NSET=EDGED,GENERATE
*ELEMENT,TYPE=S4R
*ELGEN,ELSET=SHELL
*BOUNDARY
EDGEA,ENCASTRE
EDGEB,ENCASTRE
EDGEC,ENCASTRE
EDGED,XSYMM
*SHELL SECTION,ELSET=SHELL,MATERIAL=ALUMINUM,SECTION INTEGRATION=GAUSS
.125,
**
*MATERIAL,NAME=ALUMINUM
*ELASTIC
10.5E6,0.333
*PLASTIC
4.4E4,
*DENSITY
2.5E-4,
**
*NSET,NSET=BLAST1,GENERATE
*NSET,NSET=BLAST5,GENERATE
*NSET,NSET=BLAST9,GENERATE
*NSET,NSET=BLAST13,GENERATE
*NSET,NSET=BLAST17,GENERATE
*INITIAL CONDITIONS,TYPE=VELOCITY
BLAST1, 3,-5650.
BLAST5, 3,-5575.
BLAST9, 3,-5407.
BLAST13,3,-5146.
BLAST17,3,-4893.
BLAST1, 1,-0.
BLAST5, 1,-737.
BLAST9, 1,-1463.
BLAST13,1,-2162.
BLAST17,1,-2825.
**
*ELSET, ELSET=ELOUT
*NSET,NSET=A
*STEP
*DYNAMIC,EXPLICIT
,1.E-3
*MONITOR,NODE=3201,DOF=3
***OUTPUT,HISTORY,TIME INTERVAL=0.0
***ENERGY OUTPUT
**ALLAE,ALLIE,ALLKE,ALLPD,ALLSE,ALLVD,ALLWK,ETOTAL
***ELEMENT OUTPUT,ELSET=ELOUT
**SF,STH
***ELEMENT OUTPUT,ELSET=ELOUT,SECTIONPOINT=1
**PEEQ,MISES
***ELEMENT OUTPUT,ELSET=ELOUT,SECTIONPOINT=2
**PEEQ,MISES
***ELEMENT OUTPUT,ELSET=ELOUT,SECTIONPOINT=3
**PEEQ,MISES
***NODE OUTPUT,NSET=A
**U,V
*OUTPUT,FIELD,VAR=PRESELECT,NUM=5,TIMEMARKS=NO
*ELEMENT OUTPUT,ELSET=ELOUT
 PEEQ,MISES
 SF,STH
*NODE OUTPUT
 U,V
*OUTPUT,HISTORY,OP=NEW,TIME INTERVAL=0.0
*ELEMENT OUTPUT,ELSET=ELOUT
 SF,STH
*ELEMENT OUTPUT,ELSET=ELOUT
 PEEQ,MISES
*NODE OUTPUT,NSET=A
 U,V
**
** Output requests for qa testing
**
*NSET,NSET=QA_TEST
A,
*ELSET,ELSET=QA_TEST
ELOUT,
*OUTPUT,FIELD,NUM=4,TIMEMARKS=YES
*NODE OUTPUT,NSET=QA_TEST
U,
*ELEMENT OUTPUT,ELSET=QA_TEST
PEEQ,
*OUTPUT,HISTORY,VAR=PRESELECT,TIME INTERVAL=2.5E-4
*FILE OUTPUT,NUM=4,TIMEMARKS=YES
*EL FILE, ELSET=ELOUT
 PEEQ,
*NODE FILE, NSET=A
 U,
*ENERGY FILE
*END STEP