*Heading
** Job name: elbowcolpse_shl2sld_s8r_c3d20r Model name: Model-1
**
** PARTS
**
*Part, name=Part-1
*End Part
*Part, name=Part-2
*End Part
*Part, name=Part-3
*End Part
**
** ASSEMBLY
**
*Assembly, name=Assembly
**
*Instance, name=Part-2-1, part=Part-2
*Node
*Element, type=S8R
** Region: (Section-2:Picked)
*Elset, elset=_I1, internal, generate
** Section: Section-2
*Shell Section, elset=_I1, material=Material-1
0.37, 7
*End Instance
**
*Instance, name=Part-1-1, part=Part-1
*Node
*Element, type=C3D20R
** Region: (Section-1:Picked)
*Elset, elset=_I1, internal, generate
** Section: Section-1
*Solid Section, elset=_I1, material=Material-1
1.,
*End Instance
**
*Instance, name=Part-3-1, part=Part-3
*Node
*Element, type=S8R
** Region: (Section-2:Picked)
*Elset, elset=_I1, internal, generate
** Section: Section-2
*Shell Section, elset=_I1, material=Material-1
0.37, 7
*End Instance
*Nset, nset=XSYMM1, internal, instance=Part-2-1
*Nset, nset=XSYMM1, internal, instance=Part-1-1
*Nset, nset=XSYMM1, internal, instance=Part-3-1
*Nset, nset=Load, internal, instance=Part-3-1
*Nset, nset=Fix, internal, instance=Part-2-1
*Elset, elset=_SolidToShortShell_S1, internal, instance=Part-1-1
*Elset, elset=_SolidToShortShell_S5, internal, instance=Part-1-1, generate
*Surface, type=ELEMENT, name=SolidToShortShell
 _SolidToShortShell_S1, S1
 _SolidToShortShell_S5, S5
*Elset, elset=_SolidToLongShell_S2, internal, instance=Part-1-1
*Elset, elset=_SolidToLongShell_S3, internal, instance=Part-1-1, generate
*Surface, type=ELEMENT, name=SolidToLongShell
 _SolidToLongShell_S2, S2
 _SolidToLongShell_S3, S3
*Elset, elset=_SolidInside_S5, internal, instance=Part-1-1, generate
*Surface, type=ELEMENT, name=SolidInside
 _SolidInside_S5, S5
*Elset, elset=_LongShellToSolid_E1, internal, instance=Part-2-1, generate
*Surface, type=ELEMENT, name=LongShellToSolid
 _LongShellToSolid_E1, E1
*Elset, elset=_LongShellInside_SNEG, internal, instance=Part-2-1, generate
*Surface, type=ELEMENT, name=LongShellInside
 _LongShellInside_SNEG, SNEG
*Elset, elset=_ShortShellToSolid_E3, internal, instance=Part-3-1, generate
*Surface, type=ELEMENT, name=ShortShellToSolid
 _ShortShellToSolid_E3, E3
*Elset, elset=_ShortShellInside_SNEG, internal, instance=Part-3-1, generate
*Surface, type=ELEMENT, name=ShortShellInside
 _ShortShellInside_SNEG, SNEG
*Elset, elset=_ShortShellLoad_E1, internal, instance=Part-3-1, generate
*Surface, type=ELEMENT, name=ShortShellLoad
 _ShortShellLoad_E1, E1
*Elset, elset=_LongShellFix_E3, internal, instance=Part-2-1, generate
*Surface, type=ELEMENT, name=LongShellFix
 _LongShellFix_E3, E3
** Constraint: Constraint-1
*Shell to solid coupling, constraint name=Constraint-1, influence distance=.205
 ShortShellToSolid, SolidToShortShell
** Constraint: Constraint-2
*Shell to solid coupling, constraint name=Constraint-2, influence distance=.205
 LongShellToSolid, SolidToLongShell
** Constraint: Constraint-3
*Coupling, constraint name=Constraint-3, ref node=Load, surface=ShortShellLoad
*Distributing
** Constraint: Constraint-4
*Coupling, constraint name=Constraint-4, ref node=Fix, surface=LongShellFix
*Distributing
*End Assembly
**
** MATERIALS
**
*Material, name=Material-1
*Elastic
 2.81e+07, 0.2642
*Plastic
 39440.,      0.
 50170., 0.00473
 54950., 0.01264
 58540., 0.02836
 61520.,  0.0491
 76520.,   0.105
**** ----------------------------------------------------------------
**
** STEP: Step-1
**
*Step, name=Step-1, nlgeom
 Pressurize pipe
*Static
 0.25, 1.
**
** BOUNDARY CONDITIONS
**
*Boundary
 XSYMM1, XSYMM
 Load, XSYMM
 Fix, 1,6
**
** LOADS
**
*Dsload
 LongShellInside, P, 500.
 ShortShellInside, P, 500.
 SolidInside, P, 500.
*Cload,Follower
 Load,3,-4.7882e4
**
** FIELD OUTPUT: F-Output-1
**
*Output, field, frequency = 999
*Node Output
 U, RF
*Element Output
 S, PE, PEEQ, PEMAG, LE
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, freq=0
*End Step
**** ----------------------------------------------------------------
**
** STEP: Step-2
**
*Step, name=Step-2
 Bend pipe
*Static, riks
 .1, 1.,.01,.5,2.0,Load,4,-.2
**
** BOUNDARY CONDITIONS
**
*Boundary
 Load, 4, 4, -.2
**
** FIELD OUTPUT: F-Output-1
**
*Output, field, frequency = 999
*Node Output
 U, RF
*Element Output
 S, PE, PEEQ, PEMAG, LE
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history
*Node Output, nset=Load
 U, RF
*End Step