*Heading
** Job name: Solid_Plate_01 Model name: Solid_plate
** Generated by: Abaqus/CAE 6.9-EFR
*Preprint, echo=NO, model=NO, history=NO, contact=NO
**
** PARTS
**
*Part, name=Solid-Plate
*Node
*Element, type=S4R
*Nset, nset=x0_edge, generate
*Elset, elset=x0_edge, generate
*Nset, nset=y0_edge, generate
*Elset, elset=y0_edge, generate
*Nset, nset=xL_edge, generate
*Elset, elset=xL_edge, generate
*Nset, nset=yL_edge, generate
*Elset, elset=yL_edge, generate
*Nset, nset=ALL, generate
*Elset, elset=ALL, generate
*Nset, nset=Center
*Elset, elset=_Top_Surface_SPOS, internal, generate
*Surface, type=ELEMENT, name=Top_Surface
_Top_Surface_SPOS, SPOS
*Elset, elset=_Bottom_Surface_SNEG, internal, generate
*Surface, type=ELEMENT, name=Bottom_Surface
_Bottom_Surface_SNEG, SNEG
** Section: Section-1
*Shell Section, elset=ALL, material=Steel_49Fe-24Ni-21Cr-6Mo_wt, controls=EC-1
12.7, 9
*End Part
**
**
** ASSEMBLY
**
*Assembly, name=Assembly
**
*Instance, name=Solid-Plate-1, part=Solid-Plate
*End Instance
**
*Node
*Nset, nset=BLAST-SOURCE
*Nset, nset=QA_test_Solid-Plate-Center
Solid-Plate-1.Center
**
*End Assembly
**
** ELEMENT CONTROLS
**
*Section Controls, name=EC-1, hourglass=ENHANCED
**
** MATERIALS
**
** High-ductility Stainles Steel Alloy with 49% Fe, 24%Ni, 21%Cr, 6%Mo by
** weight.
*Material, name=Steel_49Fe-24Ni-21Cr-6Mo_wt
**----------------------------------
** Material Prop. for AL-6XN Steel
**----------------------------------
*Density
 7.85e-09,
*Elastic
 161.0e+03, 0.35
*Plastic, hardening=Johnson Cook
 400.0, 1500.0, 0.40, 1.20, 1800.0, 293.0
*Rate Dependent, type=Johnson Cook
*Specific Heat
 452e+6
*Initial Condition, type=temperature
 Solid-Plate-1.ALL, 273.0
**----------------------------------
**
** BOUNDARY CONDITIONS
**
** Name: BC-x0 Type: Symmetry/Antisymmetry/Encastre
*Boundary
Solid-Plate-1.x0_edge, XSYMM
** Name: BC-xL Type: Symmetry/Antisymmetry/Encastre
*Boundary
Solid-Plate-1.xL_edge, ENCASTRE
** Name: BC-y0 Type: Symmetry/Antisymmetry/Encastre
*Boundary
Solid-Plate-1.y0_edge, YSYMM
** Name: BC-yL Type: Symmetry/Antisymmetry/Encastre
*Boundary
Solid-Plate-1.yL_edge, ENCASTRE
**
** INCIDENT WAVE PROPERTY
**
*Incident Wave Interaction Property, Name=BLAST, Type=AIR BLAST
*Conwep Charge Property
** ----------------------------------------------------------------
**
** STEP: Blast_Loading
**
*Step, name=Blast_Loading
CONWEP Blast Loading
*Dynamic, Explicit
, 1.5e-3
*Bulk Viscosity
*Incident Wave Interaction, Property=BLAST, Conwep
Solid-Plate-1.Top_Surface, Blast-Source, , 0.0, 1.0
**
** OUTPUT REQUESTS
**
*Restart, write, number interval=1, time marks=NO
**
** FIELD OUTPUT: F-Output-1
**
*Output, field, variable=PRESELECT, number inter=4
***Output, field, variable=PRESELECT, time interval=1.0e-5
*Element Output
 TEMP
**
** HISTORY OUTPUT: H-Output-2
**
*Output, history, time interval=2.5e-4
*Node Output, nset=QA_test_Solid-Plate-Center
** *Node Output, nset=Solid-Plate-1.Center
UT,
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step