*Heading
** Job name: solid-plate-c3d8r-ehg_01 Model name: Solid-Plate
** Generated by: Abaqus/CAE 6.9-EFR
*Preprint, echo=NO, model=NO, history=NO, contact=NO
**
** PARTS
**
*Part, name=Solid-Plate
*Node
*Element, type=C3D8R
*Nset, nset=ALL, generate
*Elset, elset=ALL, generate
*Nset, nset=xL, generate
*Elset, elset=xL, generate
*Nset, nset=yL, generate
*Elset, elset=yL, generate
*Nset, nset=x0, generate
*Elset, elset=x0, generate
*Nset, nset=y0, generate
*Elset, elset=y0, generate
*Nset, nset=Top-Center
*Nset, nset=Bot-Center
*Elset, elset=_Top-Surf_S3, internal
*Surface, type=ELEMENT, name=Top-Surf
_Top-Surf_S3, S3
*Elset, elset=_Bottom-Surf_S5, internal
*Surface, type=ELEMENT, name=Bottom-Surf
_Bottom-Surf_S5, S5
** Section: AL-6XN_Section
*Solid Section, elset=ALL, controls=EC-1, material=Al-6XN
*End Part
**
**
** ASSEMBLY
**
*Assembly, name=Assembly
**
*Instance, name=Solid-Plate-1, part=Solid-Plate
*End Instance
**
*Node
*Nset, nset=Blast-Source
*Nset, nset=QA_test_Top-Center
 Solid-Plate-1.Top-Center
*Nset, nset=QA_test_Bot-Center
 Solid-Plate-1.Bot-Center
*End Assembly
**
** ELEMENT CONTROLS
**
*Section Controls, name=EC-1, hourglass=ENHANCED
**
** MATERIALS
**
** High ductility stainless steel alloy (AL-6XN) with approximate composition of
** 49Fe-24Ni-21Cr-6Mo by weight
*Material, name=Al-6XN
*Density
 7.85e-09,
*Elastic
161000., 0.35
*Expansion
452.,
*Plastic, hardening=JOHNSON COOK
400.,1500.,  0.4,  1.2,1800., 293.
*Rate Dependent, type=JOHNSON COOK
**
** BOUNDARY CONDITIONS
**
** Name: BC-x0 Type: Symmetry/Antisymmetry/Encastre
*Boundary
Solid-Plate-1.x0, XSYMM
** Name: BC-xL Type: Symmetry/Antisymmetry/Encastre
*Boundary
Solid-Plate-1.xL, ENCASTRE
** Name: BC-y0 Type: Symmetry/Antisymmetry/Encastre
*Boundary
Solid-Plate-1.y0, YSYMM
** Name: BC-yL Type: Symmetry/Antisymmetry/Encastre
*Boundary
Solid-Plate-1.yL, ENCASTRE
**
** PREDEFINED FIELDS
**
** Name: Temperature   Type: Temperature
*Initial Conditions, type=TEMPERATURE
Solid-Plate-1.ALL, 273.
**
** INCIDENT WAVE PROPERTY
**
*Incident Wave Interaction Property, Name=BLAST, Type=AIR BLAST
*Conwep Charge Property
** ----------------------------------------------------------------
**
** STEP: Blast-Loading
**
*Step, name=Blast-Loading
Conwep Blast Loading
*Dynamic, Explicit
, 0.0015
*Bulk Viscosity
**
** INCIDENT WAVE INTERACTION
**
*Incident Wave Interaction, Property=BLAST, Conwep
Solid-Plate-1.Top-Surf, Blast-Source, , 0.0, 1.0
**
** OUTPUT REQUESTS
**
*Restart, write, number interval=1, time marks=NO
**
** FIELD OUTPUT: F-Output-1
**
*Output, field, variable=PRESELECT, number inter=4
**
** HISTORY OUTPUT: Top-Center-History
**
*Output, history, time interval=2.5e-4
*Node Output, nset=QA_test_Top-Center
** *Node Output, nset=Solid-Plate-1.Top-Center
UT,
**
** HISTORY OUTPUT: Bot-Center-History
**
*Output, history, time interval=2.5e-4
*Node Output, nset=QA_test_Bot-Center
** *Node Output, nset=Solid-Plate-1.Bot-Center
UT,
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step