*Heading
*Post Output, Step=1
*Output, field
*Node Output
 U,
*Output, history
*Node Output, nset=Beam1End
 RF,
*Node Print, nset=Beam1End
 RF,
*Node Print, nset=Beam2End
 RF,
*Post Output, Step=7
*Output, field
*Node Output
 U,
*Output, history
*Node Output, nset=Beam1End
 RF,
*Node Print, nset=Beam1End
 RF,
*Node Print, nset=Beam2End
 RF,