*HEADING
FeFp: c3d8rh, uniaxial tension, orientation
Marlow model, incompressible, mullins effect
*NODE,NSET=one
*NSET,NSET=FACE1
*NSET,NSET=FACE2
*NSET,NSET=FACE3
*NSET,NSET=FACE4
*NSET,NSET=FACE5
*NSET,NSET=FACE6
*nset,nset=noutu
*nset,nset=noutf
*ELEMENT,TYPE=C3D8rH,ELSET=ONE
*orientation,name=ori1
*SOLID SECTION,ELSET=ONE,MATERIAL=mat-129,ori=ori1
*MATERIAL,NAME=mat-129
*HYPERELASTIC,marlow,poisson=0.5
*include, input=heplmu_matprops_uni.inp
*amplitude,name=cl1
0.0,0.0, 10.,1.413142, 20.0,0.0, 40.,2.150516
60.,0.0, 90.0,5.23807
*STEP,NLGEOM,INC=2000
*STATIC
1.0,90.,,1.0
*BOUNDARY
FACE1,3
FACE3,2
FACE6,1
*cload, amplitude=cl1
face4,1,0.25
*output,history,freq=1
*node output,nset=noutu
u1
*node output,nset=noutf
rf1
*output,field,freq=200
*node output
u
*element output
s
*END STEP