*HEADING
FeFp: c3d8rh, simple shear, orientation
Ogden, incompressible, mullins effect
Uniaxial and biaxial test data for input
*NODE,NSET=one
*NSET,NSET=FACE1
*NSET,NSET=FACE2
*NSET,NSET=FACE3
*NSET,NSET=FACE4
*NSET,NSET=FACE5
*NSET,NSET=FACE6
*ELEMENT,TYPE=C3D8H,ELSET=ONE
*orientation, name=ori1
*SOLID SECTION,ELSET=ONE,MATERIAL=mat-129,ori=ori1
*MATERIAL,NAME=mat-129
*HYPERELASTIC,ogden, n=3,test
*include, input=heplmu_matprops.inp
*amplitude,name=nominal_strain
0.0,0.0, 10.,0.4, 20.,0.0, 40.,0.8,
50.,0.0, 70.,1.6
*STEP,NLGEOM,INC=2000
*STATIC
0.5,70.,,0.5
*BOUNDARY
FACE6,1,3
FACE4,1,1
*boundary, amplitude=nominal_strain
face4,3,3,1.0
*output,field,freq=300
*node output
u
*output,history,freq=1
*node output,nset=FACE6
rf
*node output,nset=FACE4
u
*output, field, var=pre
*END STEP