*HEADING
 TEST OF SUBSTRUCTURE MATRIX OUTPUT
 READS AND USES SUBSTRUCTURE MATRIX WRITTEN TO THE RESULTS FILE IN
 indianpoint_3sub_gen1.inp, indianpoint_3sub_gen2.inp and indianpoint_3sub_gen3.inp
*NODE
*NGEN
*NGEN,LINE=C
*NODE
*NGEN
*NGEN,LINE=C
*NODE
*NGEN
*NGEN,LINE=C
**
** SPRING DEFINITIONS
**
*NODE,NSET=SPRS
*NSET,NSET=NPDR
*ELEMENT,TYPE=SPRINGA,ELSET=FWR11
*ELEMENT,TYPE=SPRINGA,ELSET=FWR13
*ELEMENT,TYPE=SPRINGA,ELSET=FWR14
*ELEMENT,TYPE=SPRINGA,ELSET=FWR17
*ELEMENT,TYPE=SPRINGA,ELSET=FWR18
*ELEMENT,TYPE=SPRINGA,ELSET=FWR20
*ELEMENT,TYPE=SPRINGA,ELSET=FWR21
*ELEMENT,TYPE=SPRINGA,ELSET=FWR23
*ELEMENT,TYPE=SPRINGA,ELSET=FWR25
*ELEMENT,TYPE=SPRINGA,ELSET=FWR24
*ELEMENT,TYPE=SPRINGA,ELSET=FWR27
*ELEMENT,TYPE=SPRINGA,ELSET=FWR28
*ELSET,ELSET=SPRINGS
FWR11, FWR13, FWR14, FWR17, FWR18, FWR20,
FWR21, FWR23, FWR24,  FWR25, FWR27, FWR28
*SPRING,ELSET=FWR11
17700.,
*SPRING,ELSET=FWR13
119600.,
*SPRING,ELSET=FWR14
403000.,
*SPRING,ELSET=FWR17
97900.,
*SPRING,ELSET=FWR18
228000.,
*SPRING,ELSET=FWR20
86300.,
*SPRING,ELSET=FWR21
86300.,
*SPRING,ELSET=FWR23
319000.,
*SPRING,ELSET=FWR24
56800.,
*SPRING,ELSET=FWR25
39100.,
*SPRING,ELSET=FWR27
55500.,
*SPRING,ELSET=FWR28
68000.,
*USER ELEMENT,TYPE=U01,FILE=indianpoint_3sub_gen1,OLD ELEMENT=Z01
*USER ELEMENT,TYPE=U02,FILE=indianpoint_3sub_gen2,OLD ELEMENT=Z02
*USER ELEMENT,TYPE=U03,FILE=indianpoint_3sub_gen3,OLD ELEMENT=Z03
*ELEMENT,TYPE=U01,ELSET=UALL
*ELEMENT,TYPE=U02,ELSET=UALL
*ELEMENT,TYPE=U03,ELSET=UALL
*UEL PROPERTY,ELSET=UALL
*BOUNDARY
1,1,6
76,1,6
70,1
70,2
10,2
SPRS,1,3
*NSET,NSET=SUP1
*NSET,NSET=SUP2
*NSET,NSET=SUP3
*NSET,NSET=SUPALL
SUP1,SUP2,SUP3
*NSET,NSET=SMALL
*STEP
     FREQUENCY EXTRACTION
*FREQUENCY, eigensolver=lanczos, SIM=NO
24, ,
*MODAL FILE
*END STEP
*STEP,PERTURBATION
  SNAP LOAD---APPLIED STATICALLY
*STATIC
*EL PRINT,ELSET=SPRINGS
S,E
*CLOAD
25,3,7000.
*NODE PRINT,NSET=SMALL,FREQUENCY=100
U,
*END STEP
*STEP
 RELEASE LOAD
*MODAL DYNAMIC,CONTINUE=YES
 0.02,10.0
*MODAL DAMPING,MODAL=DIRECT
*SELECT EIGENMODES, GENERATE
*PRINT,FREQUENCY=100
*EL FILE,ELSET=SPRINGS,FREQUENCY=100
S,
*NODE FILE,NSET=SMALL,FREQUENCY=100
U,
V,
A    ,      ,      ,      ,
*NODE PRINT,NSET=SMALL,FREQUENCY=100
U,
*EL PRINT,ELSET=SPRINGS,FREQUENCY=100
S,
*OUTPUT,FIELD, FREQUENCY=999
*ELEMENT OUTPUT,ELSET=SPRINGS
S,
*NODE OUTPUT,NSET=SMALL
U,
V,
A ,
*OUTPUT,HISTORY,FREQUENCY=100
*ELEMENT OUTPUT,ELSET=SPRINGS
S,
*NODE OUTPUT,NSET=SMALL
U,
V,
A    ,      ,      ,      ,
*END STEP