*HEADING
 INDIAN  POINT FEEDWATER LINE WITH SPRING SUPPORT
RESTART
*RESTART,READ,STEP=1
*STEP
*FREQUENCY,EIGENSOLVER=LANCZOS, SIM=NO
15,25.0,50.0
*BOUNDARY,OP=NEW
1,1,3
76,1,6
70,1
70,2
10,2
SPRS,1,3
*EL PRINT,FREQUENCY=0
*EL FILE,ELSET=SPRINGS
ELEN,
*EL FILE,ELSET=ONE
ENER,
ELEN,
*NODE PRINT,FREQUENCY=0
*OUTPUT,HISTORY
*ELEMENT OUTPUT,ELSET=ONE
ENER,
ELEN,
*END STEP