*HEADING
 INDIAN  POINT FEEDWATER LINE WITH SPRING SUPPORTS
*RESTART,READ,STEP=1
*STEP
*FREQUENCY,EIGENSOLVER=LANCZOS, SIM=NO
15,25.0,60.0
*EL PRINT,FREQUENCY=0
*EL FILE,ELSET=SPRINGS
ELEN,
*EL FILE,ELSET=ONE
ENER,
ELEN,
*NODE PRINT,FREQUENCY=0
*OUTPUT,HISTORY
*ELEMENT OUTPUT,ELSET=ONE
ENER,
ELEN,
*END STEP