*HEADING
CAST IRON PLASTICITY, SHEAR, C3D8
*IMPORT,STEP=1,STATE=YES,UPDATE=NO
ONE
*NSET,NSET=FACE1
*NSET,NSET=FACE2
*NSET,NSET=FACE3
*NSET,NSET=FACE4
*NSET,NSET=FACE42
*NSET,NSET=FACE5
*NSET,NSET=FACE6
*EQUATION
FACE42,1,1, 2,1,-1
*EQUATION
*EQUATION
*STEP
Step 1: Shear
*DYNAMIC,EXPLICIT
 ,1.
*BOUNDARY,OP=NEW,TYPE=VELOCITY
FACE6,1,1
1,2,2,
5,2,2,
FACE2,3,3
2,2,2,0.0075
6,2,2,0.0075
*OUTPUT,FIELD
*NODE OUTPUT
U,RF
*ELEMENT OUTPUT
S,LE,PE
PEEQT,PEEQ
*OUTPUT,HISTORY
*ELEMENT OUTPUT, ELSET=ONE
PRESS,MISES,S,E,PE
PEEQT,PEEQ
*RESTART,WRITE
*END STEP