*HEADING
 STEADY-STATE ROLLING ANALYSIS OF A TIRE
 STEP 0: RESTART FROM ROLLINGTIRE_BRAKE_TRAC
 STEP 1: GET EQUILIBRIUM
 STEP 2: SEARCH FREE ROLLING STATE
 UNITS: KG, M
*RESTART,READ,STEP=3,INC=8,END STEP,WRITE,FREQ=2
*FILE FORMAT,ZERO INCREMENT
***************************************************
*STEP,INC=300,NLGEOM,UNSYMM=YES
 1:  STRAIGHT LINE ROLLING
*STEADY STATE TRANSPORT, LONG TERM
*TRANSPORT VELOCITY
 NTIRE, 9.00
*END STEP
***************************************************
*STEP,INC=300,NLGEOM,UNSYMM=YES
 2:  STRAIGHT LINE ROLLING  (Partial traction)
*STEADY STATE TRANSPORT, LONG TERM
*TRANSPORT VELOCITY
 NTIRE, 9.04
*END STEP