*HEADING
UNLOADING OF SHALLOW ARCH
*RESTART, READ, STEP=1, INC=12, WRITE, FREQUENCY=0,
END STEP
*STEP,NLGEOM
*STATIC,RIKS
.05,1.,,,,1,2,0.
*DSLOAD
SURFACE,P,-4685.6
*END STEP