*heading
Import S2X: Explicit job, c3d8r
simple shear with orientation
*restart,write,num=20
*IMPORT,STEP=1,inc=40,UPDATE=no,STATE=YES
 ONE
*amplitude,name=ne2
0.,0.0, 0.02,0.6, 0.03,0.0, 0.05,1.0
*STEP,nlgeom=yes
*dynamic,explicit
,0.05,,
*BOUNDARY
FACE6,1,3
FACE4,1,2
*boundary, amplitude=ne2
face4,3,3,1.0
*output,field
*node output
u
*output,history,freq=1
*node output,nset=FACE6
rf
*node output,nset=FACE4
u
*END STEP