*HEADING
 Test import capability with FeFp: Standard to Explicit
 Element: CPS4R + orientation
 Material: marlow + plasticity + mullins
 Results imported from: sx_s_fefp2d_biori.inp
**
*IMPORT,STEP=1,inc=20,UPDATE=no,STATE=YES
 solid
**
*amplitude,name=ne3
 0.0, 0.0, 0.25, 1.0, 0.5, 1.2, 1., 0.0
**------------------------
*STEP
*dynamic,explicit
 ,1.,
*BOUNDARY
 x0,1
 y0,2
*boundary, amplitude=ne3
 x1,1,1,0.4
 y1,2,2,0.2
*output,field
*node output
u
RF
*element output
S
PEEQ
E
*output,history,time interval=0.01
*element output,elset=solid
 s11,
 s22,
 LE11
*END STEP