*ELSET,ELSET=BUMPER-MTG-FRONT-LT,GEN
*SURFACE,NAME=BUMPER-MTG-FRONT-LT,TYPE=ELEMENT
BUMPER-MTG-FRONT-LT,SPOS
*COUPLING,REF NODE=111380,SURFACE=BUMPER-MTG-FRONT-LT,CONSTRAINT NAME=BUMPER-MTG-FRONT-LT
*DISTRIBUTING
***************************************
*ELSET,ELSET=BUMPER-MTG-S-LT,GEN
*SURFACE,NAME=BUMPER-MTG-S-LT,TYPE=ELEMENT
BUMPER-MTG-S-LT,SPOS
*COUPLING,REF NODE=111794,SURFACE=BUMPER-MTG-S-LT,CONSTRAINT NAME=BUMPER-MTG-S-LT
*DISTRIBUTING
*************************************
*ELSET,ELSET=BUMPER-MTG-FRONT-RT
*SURFACE,NAME=BUMPER-MTG-FRONT-RIGHT,TYPE=ELEMENT
BUMPER-MTG-FRONT-RT,SPOS
*COUPLING,REF NODE=111475,SURFACE=BUMPER-MTG-FRONT-RIGHT,CONSTRAINT NAME=BUMPER-MTG-FRONT-RIGHT
*DISTRIBUTING
***********************************
*ELSET,ELSET=BUMPER-MTG-S-RT,GEN
*SURFACE,NAME=BUMPER-MTG-S-RT,TYPE=ELEMENT
BUMPER-MTG-S-RT,SPOS
*COUPLING,REF NODE=112195,SURFACE=BUMPER-MTG-S-RT,CONSTRAINT NAME=BUMPER-MTG-S-RT
*DISTRIBUTING
**************************************************************************
** add dummy mass/rotary inertia to coupling ref nodes
*ELEMENT, TYPE=MASS, ELSET=bumper_mass
*MASS, ELSET=bumper_mass
<small_mass>,
*ELEMENT, TYPE=ROTARYI, ELSET=bumper_rotary
*ROTARY INERTIA, ELSET=bumper_rotary
<small_rota>,<small_rota>,<small_rota>
**************************************************************************
*nset,nset=retained_bumper,unsorted
*nset,nset=retained_all
retained_bumper
**