**--------------------------------------------------------
**- internal MPCs to cabin
*NSET,NSET=radiator-BL,GEN
*NSET,NSET=radiator-BR,GEN
*NSET,NSET=radiator-TL,GEN
*NSET,NSET=radiator-TR,GEN
*MPC
BEAM,radiator-BL,9000001
BEAM,radiator-BR,9000002
BEAM,radiator-TL,9000003
BEAM,radiator-TR, 9000004
**--------------------------------------------------------
*ELSET,ELSET=CABIN-D-HINGE-UP-LT,GEN
*SURFACE,NAME=CABIN-D-HINGE-UP-LT,TYPE=ELEMENT
CABIN-D-HINGE-UP-LEFT,SNEG
*COUPLING,REF NODE=9000011,SURFACE=CABIN-D-HINGE-UP-LT,CONSTRAINT NAME=CABIND-D-HINGE-UP-LT
*DISTRIBUTING
**********************************************************
*ELSET,ELSET=CABIN-D-HINGE-LOW-LT,GEN
*SURFACE,NAME=CABIN-D-HINGE-LOW-LT,TYPE=ELEMENT
CABIN-D-HINGE-LOW-LEFT,SNEG
*COUPLING,REF NODE=9000009,SURFACE=CABIN-D-HINGE-LOW-LT,CONSTRAINT NAME=CABIN-D-HINGE-LOW-LT
*DISTRIBUTING
*********************************************************
*ELSET,ELSET=CABIN-DOORJAMP-LT
*SURFACE,NAME=DOOR-CLOSURE-IN-LT,TYPE=ELEMENT
DOOR-CLOSURE-IN-LEFT,SNEG
*SURFACE,NAME=CABIN-DOORJAMP-LT,TYPE=ELEMENT
CABIN-DOORJAMP-LT,SNEG
*TIE,NAME=DOOR-CLOSURE-IN-LT-DOORJAMP,POSITION TOLERANCE=100
DOOR-CLOSURE-IN-LT,CABIN-DOORJAMP-LT
*COUPLING,REF NODE=1800291,SURFACE=CABIN-DOORJAMP-LT,CONSTRAINT NAME=CABIN-DOORJAMP-LT
*DISTRIBUTING
**************************************************
*ELSET,ELSET=CABIN-D-HINGE-UP-RT,GEN
*SURFACE,NAME=CABIN-D-HINGE-UP-RT,TYPE=ELEMENT
CABIN-D-HINGE-UP-RIGHT,SNEG
*COUPLING,REF NODE=9000005,SURFACE=CABIN-D-HINGE-UP-RT,CONSTRAINT NAME=CABIN-D-HINGE-UP-RT
*DISTRIBUTING
***************************************************
*ELSET,ELSET=CABIN-D-HINGE-LOW-RT,GEN
*SURFACE,NAME=CABIN-D-HINGE-LOW-RT,TYPE=ELEMENT
CABIN-D-HINGE-LOW-RIGHT,SNEG
*COUPLING,REF NODE=9000007,SURFACE=CABIN-D-HINGE-LOW-RT,CONSTRAINT NAME=CABIN-D-HINGE-LOW-RT
*DISTRIBUTING
*******************************************
*ELSET,ELSET=CABIN-DOORJAMP-RT
*SURFACE,NAME=CABIN-DOORJAMP-RT,TYPE=ELEMENT
CABIN-DOORJAMP-RT,SNEG
*SURFACE,NAME=DOOR-CLOSURE-IN-RT,TYPE=ELEMENT
DOOR-CLOSURE-IN-RIGHT,SPOS
*TIE,NAME=DOOR-CLOSURE-IN-RT-DOORJAMP,POSITION TOLERANCE=100
DOOR-CLOSURE-IN-RT,CABIN-DOORJAMP-RT
*COUPLING,REF NODE=1800142,SURFACE=CABIN-DOORJAMP-RT,CONSTRAINT NAME=CABIN-DOORJAMP-RT
*DISTRIBUTING
***********************************************************************
******CABIN-MTG-FRONT-LEFT TO LEFT RAIL CONNECTION ********************
***********************************************************************
*ELSET,ELSET=CABIN-MTG-REINF-FRONT-LT
*SURFACE,NAME=CABIN-MTG-REINF-FRONT-LT,TYPE=ELEMENT
CABIN-MTG-REINF-FRONT-LT,SPOS
*COUPLING,REF NODE=181576,SURFACE=CABIN-MTG-REINF-FRONT-LT,CONSTRAINT NAME=CABIN-MTG-REINF-FRONT-LT
*DISTRIBUTING
***************************************************
*ELSET,ELSET=CABIN-MTG-REINF-FRONT-RT
*SURFACE,NAME=CABIN-MTG-REINF-FRONT-RT,TYPE=ELEMENT
CABIN-MTG-REINF-FRONT-RT,SPOS
*COUPLING,REF NODE=124109,SURFACE=CABIN-MTG-REINF-FRONT-RT,CONSTRAINT NAME=CABIN-MTG-REINF-FRONT-RT
*DISTRIBUTING
*****************************************************
*ELSET,ELSET=CABIN-MTG-REINF-RIGHT-LT
*SURFACE,NAME=CABIN-MTG-REINF-RIGHT-LT,TYPE=ELEMENT
CABIN-MTG-REINF-RIGHT-LT,SPOS
*COUPLING,REF NODE=181661,SURFACE=CABIN-MTG-REINF-RIGHT-LT,CONSTRAINT NAME=CABIN-MTG-REINF-RIGHT-LT
*DISTRIBUTING
**********************************************************
*ELSET,ELSET=CABIN-MTG-REINF-RIGHT-RT
*SURFACE,NAME=CABIN-MTG-REINF-RIGHT-RT,TYPE=ELEMENT
CABIN-MTG-REINF-RIGHT-RT,SPOS
*COUPLING,REF NODE=125059,SURFACE=CABIN-MTG-REINF-RIGHT-RT,CONSTRAINT NAME=CABIN-MTG-REINF-RIGHT-RT
*DISTRIBUTING
*****************************************************
*ELSET,ELSET=RADIATOR-MTG-M-LT
*SURFACE,NAME=RADIATOR-MTG-M-LT
RADIATOR-MTG-M-LT,SPOS
*COUPLING,REF NODE=158003,SURFACE=RADIATOR-MTG-M-LT,CONSTRAINT NAME=RADIATOR-MTG-M-LT
*DISTRIBUTING
*************************************************************
*ELSET,ELSET=RADIATOR-MTG-M-RT
*SURFACE,NAME=RADIATOR-MTG-M-RT
RADIATOR-MTG-M-RT,SPOS
*COUPLING,REF NODE=158521,SURFACE=RADIATOR-MTG-M-RT,CONSTRAINT NAME=RADIATOR-MTG-M-RT
*DISTRIBUTING
*********************************************
*ELSET,ELSET=HOOD-HINGE-2-LT
*SURFACE,NAME=HOOD-HINGE-2-LT,TYPE=ELEMENT
HOOD-HINGE-2-LT,SPOS
*COUPLING,REF NODE=284775,SURFACE=HOOD-HINGE-2-LT,CONSTRAINT NAME=HOOD-HINGE-2-LT
*DISTRIBUTING
**********************************************
*ELSET,ELSET=HOOD-HINGE-2-RT
*SURFACE,NAME=HOOD-HINGE-2-RT,TYPE=ELEMENT
HOOD-HINGE-2-RT,SPOS
*COUPLING,REF NODE=284140,SURFACE=HOOD-HINGE-2-RT,CONSTRAINT NAME=HOOD-HINGE-2-RT
*DISTRIBUTING
************************************************
*ELSET,ELSET=HOOD-AXIAL-CONN
*SURFACE,NAME=HOOD-AXIAL-CONN,TYPE=ELEMENT
HOOD-AXIAL-CONN,SPOS
*COUPLING,REF NODE=1810218,SURFACE=HOOD-AXIAL-CONN,CONSTRAINT NAME=HOOD-AXIAL-CONN
*DISTRIBUTING
************************************************
*elset,elset=STEER-COLUMN-SMALL,generate
*SURFACE,NAME=STEER-COLUMN,TYPE=ELEMENT
STEER-COLUMN-SMALL,SPOS
*COUPLING,REF NODE=1590000,SURFACE=STEER-COLUMN,CONSTRAINT NAME=STEER-COLUMN
*DISTRIBUTING
*nset, nset=nodeset-34
*MPC
BEAM, nodeSet-34, 1590000
***************************************************
*SURFACE,NAME=ACCELEROMETER-CG,TYPE=ELEMENT
ACCELEROMETER-CG,S2
*COUPLING,REF NODE=1990460,SURFACE=ACCELEROMETER-CG,CONSTRAINT NAME=ACCELEROMETER-CG
*DISTRIBUTING
*NSET, NSET=nodeSet-47
*MPC
BEAM, nodeSet-47,1990460
********************************************************
*ELSET,ELSET=SEAT-TRK-FRONT-RT-CABIN-BOT
*SURFACE,NAME=SEAT-TRK-FRONT-RT-CABIN-BOT,TYPE=ELEMENT
SEAT-TRK-FRONT-RT-CABIN-BOT,SPOS
*COUPLING,REF NODE=128564,SURFACE=SEAT-TRK-FRONT-RT-CABIN-BOT,CONSTRAINT NAME=SEAT-TRK-FRONT-RT-CABIN-BOT
*DISTRIBUTING
**************************************
*ELSET,ELSET=SEAT-TRK-REAR-RT-CABIN-BOT
*SURFACE,NAME=SEAT-TRK-REAR-RT-CABIN-BOT,TYPE=ELEMENT
SEAT-TRK-REAR-RT-CABIN-BOT,SPOS
*COUPLING,REF NODE=128552,SURFACE=SEAT-TRK-REAR-RT-CABIN-BOT,CONSTRAINT NAME=SEAT-TRK-REAR-RT-CABIN-BOT
*DISTRIBUTING
******************************************************
*ELSET,ELSET=SEAT-TRK-FRONT-LT-CABIN-BOT
*SURFACE,NAME=SEAT-TRK-FRONT-LT-CABIN-BOT,TYPE=ELEMENT
SEAT-TRK-FRONT-LT-CABIN-BOT,SPOS
*COUPLING,REF NODE=128064,SURFACE=SEAT-TRK-FRONT-LT-CABIN-BOT,CONSTRAINT NAME=SEAT-TRK-FRONT-LT-CABIN-BOT
*DISTRIBUTING
******************************************************
*ELSET,ELSET=SEAT-TRK-REAR-LT-CABIN-BOT
*SURFACE,NAME=SEAT-TRK-REAR-LT-CABIN-BOT,TYPE=ELEMENT
SEAT-TRK-REAR-LT-CABIN-BOT,SPOS
*COUPLING,REF NODE=128052,SURFACE=SEAT-TRK-REAR-LT-CABIN-BOT,CONSTRAINT NAME=SEAT-TRK-REAR-LT-CABIN-BOT
*DISTRIBUTING
****************************************************************************
** add dummy mass/rotary inertia to coupling ref nodes
*ELEMENT, TYPE=MASS, ELSET=cabin_mass
*MASS, ELSET=cabin_mass
<small_mass>,
*ELEMENT, TYPE=ROTARYI, ELSET=cabin_rotary
*ROTARY INERTIA, ELSET=cabin_rotary
<small_rota>,<small_rota>,<small_rota>
****************************************************************************
*nset,nset=retained_cabin_chassis,unsorted
*nset,nset=retained_cabin_radiator_chassis,unsorted
*nset,nset=retained_cabin_door_left,unsorted
*nset,nset=retained_cabin_door_right,unsorted
*nset,nset=retained_cabin_hood,unsorted
*nset,nset=retained_cabin_seat,unsorted
*nset,nset=retained_cabin_cg
**
*nset,nset=retained_cabin,unsorted
*nset,nset=retained_all
retained_cabin,
**