**---------------------------------------------------------------
**
**                  DOOR HINGES LEFT AND CABIN
**
**---------------------------------------------------------------
*ORIENTATION,NAME=ori_conn_door_left
*ELEMENT, TYPE=CONN3D2, ELSET=conn_door_hinge_left_cabin
** LOW
** UP
*CONNECTOR SECTION, ELSET=conn_door_hinge_left_cabin, BEHAVIOR=conn_door_hinges_beh
**join,align
join,revolute
ori_conn_door_left,
*CONNECTOR BEHAVIOR, NAME=conn_door_hinges_beh
*CONNECTOR ELASTICITY,COMPONENT=4
<conelPrevDoor>,
**---------------------------------------------------------------
**
**                  DOOR LOCK LEFT AND CABIN
**
**---------------------------------------------------------------
*ELEMENT, TYPE=CONN3D2, ELSET=conn_door_lock_left_cabin_cart
*CONNECTOR SECTION, ELSET=conn_door_lock_left_cabin_cart
cartesian,cardan
ori_conn_door_left,
*ELEMENT, TYPE=CONN3D2, ELSET=conn_door_lock_left_cabin
*CONNECTOR SECTION, ELSET=conn_door_lock_left_cabin
axial,
**---------------------------------------------------------------
*elset,elset=conn_all
conn_door_hinge_left_cabin,
conn_door_lock_left_cabin_cart,conn_door_lock_left_cabin
**