*include,input=tr_all_nodes.inp
*include,input=tr_parameters_inphase.inp
*include,input=tr_parameters.inp
*include,input=tr_materials.inp
*include,input=tr_susp_upper_arm_right_elts.inp
*include,input=tr_susp_upper_arm_right_coup.inp
**---------------------------------
*step
*frequency,eigen=lanc, SIM=NO
<neigenmodes>,
*boundary
retained_upper_arm_right,1,6
*end step
**-----------------------------------
*step
*substructure generate, type=z15, overwrite,
recovery matrix=<recov_yes_no>, mass matrix=yes,grav=yes,
libr=tr_suspension
**
**
*RETAINED NODAL DOFS,sorted=no
retained_upper_arm_right,
*SELECT EIGENMODES,generate
1,<neigenmodes>,1
**
**
*substructure matrix output, stiffness=yes,
mass=yes, recovery=no,grav=yes,
file=lib_upper_arm_right
*end step
**-----------------------------------