*ELSET,ELSET=INNER-BACK-RT-RIM-COUP,GEN
*SURFACE,TYPE=ELEMENT,NAME=INNER-BACK-RT-RIM-COUP
INNER-BACK-RT-RIM-COUP,SNEG
*COUPLING,REF NODE=982002,SURFACE=INNER-BACK-RT-RIM-COUP,CONSTRAINT NAME=INNER-BACK-RT-RIM-COUP
*DISTRIBUTING
**--------------------------------------------------------------
** add dummy mass/rotary inertia to coupling ref nodes
*ELEMENT, TYPE=MASS, ELSET=wheel_back_right_mass
*MASS, ELSET=wheel_back_right_mass
<small_mass>,
*ELEMENT, TYPE=ROTARYI, ELSET=wheel_back_right_rotary
*ROTARY INERTIA, ELSET=wheel_back_right_rotary
<small_rota>,<small_rota>,<small_rota>
**--------------------------------------------------------------
*nset,nset=retained_wheel_back_right,unsorted
*nset,nset=retained_all
retained_wheel_back_right,
**