*Heading
 Fung model processed through VUANISOHYPER_INV
**
*Preprint, echo=NO, model=NO, history=NO, contact=NO
*Node
*Element, type=C3D8, elset=einv44
*Element, type=C3D8, elset=einv45
*Element, type=C3D8, elset=fung
*Elset, elset=alle
*Elset, elset=QA_TEST
 alle
*Solid Section, elset=einv44, material=vuaniso_funginv44,orientation=ori-1
 1.
*Solid Section, elset=einv45, material=vuaniso_funginv45,orientation=ori-1
 1.
*Solid Section, elset=fung, material=fung,orientation=ori-1
 1.
*Nset, nset=y0, generate
*Nset, nset=x0, generate
*Nset, nset=z0
*Nset, nset=x1, generate
*Nset, nset=z1
*Nset, nset=y1, generate
**
** MATERIALS
**
*orientation,name=ori-1,local directions=3
**
*parameter
 zero = 0.0
**
 c = 26.95e3
 d = 1.e-8
 b1 = 0.9925
 b2 = 0.4180
 b3 = 0.0089
 b4 = 0.0749
 b5 = 0.0295
 b6 = 0.0193
 b7 = 5.0000
 b8 = b7
 b9 = b7
**
 b1111 = b1
 b1122 = b4
 b2222 = b2
 b1133 = b5
 b2233 = b6
 b3333 = b3
 b1212 = b7
 b1313 = b8
 b2323 = b9
**
 b1112 = zero
 b2212 = zero
 b3312 = zero
 b1113 = zero
 b2213 = zero
 b3313 = zero
 b1213 = zero
 b1123 = zero
 b2223 = zero
 b3323 = zero
 b1223 = zero
 b1323 = zero
**
 density=1.0e-1
*material,name=vuaniso_funginv44
*density
 <density>
*anisotropic hyperelastic,user,formulation=invariant, local directions=3,type=compressible,properties=23
 <b1111>,<b1122>,<b2222>,<b1133>,<b2233>,<b3333>,<b1112>,<b2212>,
 <b3312>,<b1212>,<b1113>,<b2213>,<b3313>,<b1213>,<b1313>,<b1123>,
 <b2223>,<b3323>,<b1223>,<b1323>,<b2323>,<c>,<d>
*material,name=vuaniso_funginv45
*density
 <density>
*anisotropic hyperelastic,user,formulation=invariant, local directions=3,type=compressible,properties=23
 <b1111>,<b1122>,<b2222>,<b1133>,<b2233>,<b3333>,<b1112>,<b2212>,
 <b3312>,<b1212>,<b1113>,<b2213>,<b3313>,<b1213>,<b1313>,<b1123>,
 <b2223>,<b3323>,<b1223>,<b1323>,<b2323>,<c>,<d>
*material,name=fung
*density
 <density>
*anisotropic hyperelastic,fung-anisotropic
 <b1111>,<b1122>,<b2222>,<b1133>,<b2233>,<b3333>,<b1112>,<b2212>,
 <b3312>,<b1212>,<b1113>,<b2213>,<b3313>,<b1213>,<b1313>,<b1123>,
 <b2223>,<b3323>,<b1223>,<b1323>,<b2323>,<c>,<d>
**
** ----------------------------------------------------------------
**
** STEP: Step-1
**
*boundary
 x0,1
 y0,2
 z0,3
*amplitude, name=amp-1
 0.0, 0.0, 1.0, 1.0
*Step, name=Step-1,nlgeom=yes
*dynamic,explicit
 , 1.
*cload, amplitude=amp-1
 x1,1,6000.
**
** FIELD OUTPUT
**
*Output, field, number interval=1
*element output,elset=QA_TEST
 s,le
*node output
 u,rf
**
*output,history
*element output,elset=alle
 s,le
*End Step