*heading
Import X2S: standard job, c3d8r
simple shear with orientation
*IMPORT,STEP=2,int=8,UPDATE=no,STATE=YES
 ONE
*amplitude,name=ne3
0.,0.59877, 20.,1.0, 40.,0.0
*STEP,nlgeom=yes
*static
1.e-12,1.e-12,,1.e-12
*BOUNDARY
FACE6,1,3
FACE4,1,2
*boundary,type=vel
face4,3,3,0.0
*END STEP
*STEP,nlgeom=yes
*static
0.5,40.,,0.5
*BOUNDARY
FACE6,1,3
FACE4,1,2
*boundary, amplitude=ne3
face4,3,3,1.0
*output,field,freq=10
*node output
u
*output,history,freq=1
*node output,nset=FACE6
rf
*node output,nset=FACE4
u
*END STEP