*HEADING
 Test import capability with FeFp: Explicit to Standard
 Element: CPS4R + orientation
 Material: marlow + plasticity + mullins
 Results imported from: xs_x_fefp2d_biori.inp
**
*IMPORT,STEP=1,int=5,UPDATE=no,STATE=YES
 solid
**
*amplitude,name=nominal_strain
 0.0, 0.5, 0.25, 1.0, 0.75,0.05
**------------------------
*step,nlgeom=yes
*static
 1.e-12,1.e-12
*BOUNDARY
 x0,1
 y0,2
*boundary, type=velocity
 x1,1,1,0.0
 y1,2,2,0.0
*end step
**------------------------
*STEP,nlgeom=yes
*static
0.05,1., ,0.05
*BOUNDARY
 x0,1
 y0,2
*boundary, amplitude=nominal_strain
 x1,1,1,0.4
 y1,2,2,0.2
*output,field
*node output
u
RF
*element output
S
PEEQ
E
*output,history,freq=1
*element output,elset=solid
 s11,
 s22,
 LE11
*END STEP