*heading
Import X2S - STD job
 Marlow, compressible, uniaxial
*preprint, model=yes
*IMPORT,STEP=1,int=5,UPDATE=no,STATE=YES
 ONE
*amplitude,name=nominal_strain
0.0,0.50547, 10.,1.0, 30.,0.05
*STEP,nlgeom=yes
*static
1.e-10,1.e-10,,1.e-10
*BOUNDARY
FACE1,3
FACE3,2
FACE6,1
*boundary,type=vel
face4,1,1,0.0
*END STEP
*STEP,nlgeom=yes
*static
1.,30.,,1.
*BOUNDARY
FACE1,3
FACE3,2
FACE6,1
*boundary, amplitude=nominal_strain
face4,1,1,1.0
*output,history,freq=1
*node output,nset=noutu
u1
rf1
*element output,elset=one
dmener,eldmd
*output,field
*node output,nset=one
u,rf
*element output,elset=one
s,le,pe,peeq,ener
*END STEP