*heading
*node
*element, type=conn3d2, elset=connAll
*element, type=mass, elset=mass
*mass, elset=mass
1.0e-06
*element, type=rotaryI, elset=rotary
*rotary, elset=rotary
*distribution table, name=distOriTable
 coord3d, coord3d
*distribution, name=distOri, table=distOriTable, location=element
*orientation, name=ori
 distOri
*connector section, elset=connAll
 beam
 ori, ori
*boundary
 1, 1,6
*amplitude, name=ramp, definition=smooth
0.0,0.0,10.0,1.0
*step, nlgeom=yes
*dynamic, explicit, direct
 1.e-04, 10.0
*cload, amp=ramp
** CTF1 = 1, elements 1-4
    2,    1,   -0.707107
    3,    1,   -0.707107
    4,    1,    0.707107
    5,    1,    0.707107
    2,    2,    0.707107
    3,    2,   -0.707107
    4,    2,   -0.707107
    5,    2,    0.707107
** CTF2 = 1, elements 1-4
** CTF3 = 1, elements 1-4
** CTF1 = 1, elements 5-8
** CTF2 = 1, elements 5-8
** CTF3 = 1, elements 5-8
*output, field
*element output
 CU, CTF
*end step