*HEADING
 INDIAN  POINT  WITH SPRING SUPPORTS--THREE SUBSTRUCTURE MODEL
 THIRD SUBSTRUCTURE GENERATION WITH RAYLEIGH DAMPING
**
*NODE
*NGEN
*NGEN,LINE=C
*NSET,NSET=TOP
*ELEMENT,TYPE=B31
*ELGEN,ELSET=BEAMS
*ELSET,ELSET=D8
*ELSET,ELSET=D8E
*ELSET,ELSET=BF57
*ELSET,ELSET=BWR
*ELSET,ELSET=D6
*ELSET,ELSET=D6E
*BEAM GENERAL SECTION,ELSET=D8 ,SECTION=GENERAL ,DENSITY= .0010691
12.763 , 105.317 , , 105.317 , 210.635
1. , , -1.
27.9E6 , 10.73E6
*DAMPING,ALPHA=1.5
*BEAM GENERAL SECTION,ELSET=D8E,SECTION=GENERAL  ,DENSITY=.0010691
12.763 , 50.439 , , 50.439 , 210.635
1. , , -1.
27.9E6 , 10.73E6
*DAMPING,ALPHA=1.5
*BEAM GENERAL SECTION,ELSET=D6 ,SECTION=GENERAL,DENSITY=0.00102423
8.405 , 40.295 , , 40.295 , 80.589
1.,
27.9E6 , 10.73E6
*DAMPING,ALPHA=1.5
*BEAM GENERAL SECTION,ELSET=D6E,SECTION=GENERAL ,DENSITY=0.00102423
8.405 , 21.828, ,21.828, 80.589
1.,
27.9E6 , 10.73E6
*DAMPING,ALPHA=1.5
*BEAM GENERAL SECTION,ELSET=BWR,SECTION=GENERAL  ,DENSITY=0.0013266
10.4806 , 67.143 , , 67.143 , 134.29
1. , , -1.
27.9E6 , 10.73E6
*DAMPING,ALPHA=1.5
*BEAM GENERAL SECTION,ELSET=BF57,SECTION=GENERAL ,DENSITY=0.002591
30.631 ,161.77 , , 161.77 , 323.53
1. , , -1.
27.9E6 , 10.73E6
*DAMPING,ALPHA=1.5
**
**
*STEP
*SUBSTRUCTURE GENERATE,TYPE=Z3,MASS MATRIX=YES,VISCOUS DAMPING MATRIX=YES,OVERWRITE
*RETAINED NODAL DOFS
*END STEP