*HEADING
  COMPOSITE CYLINDRICAL PANEL WITH CIRCULAR HOLE-- S9R5
**
**  FROM STUDY IN THESIS OF G.M. STANLEY
**
*RESTART,WRITE,FREQUENCY=1
*PREPRINT,ECHO=YES,MODEL=NO,HISTORY=NO
*NODE
*NGEN,NSET=OUTSIDE
**
** DEFINE CIRCLE
**
*SYSTEM
*NODE
*NGEN,LINE=C,NSET=HOLE
*SYSTEM
*NFILL,NSET=ALL
HOLE,OUTSIDE,20,100
*NSET,NSET=XPARB,GENERATE
*NSET,NSET=XPART,GENERATE
*NSET,NSET=YPAR,GENERATE
*NSET,NSET=PROFILE,GENERATE
*NMAP,TYPE=CYLINDRICAL,NSET=ALL
*EQUATION
*ELEMENT,TYPE=S9R5
*ELGEN,ELSET=ALL
*ELEMENT,TYPE=S9R5
*ELGEN,ELSET=ALL
*ELSET,ELSET=PROFILE,GENERATE
*SHELL GENERAL SECTION,ELSET=ALL
7.90239D5,2.51367D5,7.90239D5,-3.08578D-6,-7.94285D-5,2.69436D5,0.,0.
0., 4.92719D+02,0.,0.,0.,1.91513D+02,5.17951D+02,0.
0.,0.,  1.89245D+01 , 1.89245D+01 ,2.03602D+02
*BOUNDARY
XPARB,1,6
XPART,1,2
XPART,4,6
YPAR,1,2
*STEP
*BUCKLE
5,,60,20
*CLOAD
2041,3,-1000.
*EL PRINT,FREQUENCY=0
*NODE PRINT,FREQUENCY=0
*MODAL FILE
*OUTPUT,HISTORY,FREQUENCY=1
*MODAL OUTPUT
*END STEP