**---------------------------------------------------------------
**
**                  CABIN AND CHASSIS
**
**---------------------------------------------------------------
*ELEMENT, TYPE=CONN3D2, ELSET=conn_cabin_chassis
*CONNECTOR SECTION, ELSET=conn_cabin_chassis
beam,
**---------------------------------------------------------------
**
**                  RADIATOR (CABIN) AND CHASSIS
**
**---------------------------------------------------------------
*ELEMENT, TYPE=CONN3D2, ELSET=conn_radiator_cabin_chassis
*CONNECTOR SECTION, ELSET=conn_radiator_cabin_chassis
beam,
****---------------------------------------
****
****                   MEASURING CONNECTORS
****
****-----------------------------------------
*orientation,name=ori_global_cg
*element,type=conn3d2,elset=conn_yaw_pitch_roll
*connector section,elset=conn_yaw_pitch_roll
join,cardan
ori_global_cg,
*nset,nset=accelerometer-cg-shadow
**---------------------------------------
*element,type=conn3d2,elset=conn_lateral_acceleration
*connector section,elset=conn_lateral_acceleration
cartesian,
ori_global_cg,
*nset,nset=accelerometer-cg-ground
**---------------------------------------
*elset,elset=conn_all
conn_cabin_chassis,conn_radiator_cabin_chassis,
conn_yaw_pitch_roll,conn_lateral_acceleration
**