**---------------------------------------------------------------
**
**                  HOOD HINGES AND CABIN
**
**---------------------------------------------------------------
*ORIENTATION,NAME=ori_conn_hood
*ELEMENT, TYPE=CONN3D2, ELSET=conn_hood_hinges_cabin
** LEFT
** RIGHT
*CONNECTOR SECTION, ELSET=conn_hood_hinges_cabin, BEHAVIOR=conn_hood_hinges_beh
join,revolute
ori_conn_hood,
*CONNECTOR BEHAVIOR, NAME=conn_hood_hinges_beh
*CONNECTOR ELASTICITY,COMPONENT=4
<conelPrevHood>
**---------------------------------------------------------------
**
**                  HOOD LOCK AND CABIN
**
**---------------------------------------------------------------
*ELEMENT, TYPE=CONN3D2, ELSET=conn_hood_lock_cabin_cart
*CONNECTOR SECTION, ELSET=conn_hood_lock_cabin_cart
cartesian,cardan
ori_conn_hood,
*ELEMENT, TYPE=CONN3D2, ELSET=conn_hood_lock_cabin
*CONNECTOR SECTION, ELSET=conn_hood_lock_cabin
axial,
**---------------------------------------------------------------
*elset,elset=conn_all
conn_hood_hinges_cabin,
conn_hood_lock_cabin_cart,conn_hood_lock_cabin
**