**---------------------------------------
*element,type=conn3d2,elset=conn_steer_left
*connector section,elset=conn_steer_left
join,
**
*ORIENTATION,NAME=conn_tie_rod_prevRigRot_left
*element,type=conn3d2,elset=conn_tie_rod_prevRigRot_left
*connector section, elset=conn_tie_rod_prevRigRot_left,behavior=conn_tie_rod_prevRigRot_left
join,cardan
conn_tie_rod_prevRigRot_left,
*connector behavior, name=conn_tie_rod_prevRigRot_left
*connector elasticity,comp=4
<conelPrevSteer>,
*connector elasticity,comp=5
<conelPrevSteer>,
*connector elasticity,comp=6
<conelPrevSteer>,
**---------------------------------------
*element,type=conn3d2,elset=conn_steer_right
*connector section,elset=conn_steer_right
join,
**
*ORIENTATION,NAME=conn_tie_rod_prevRigRot_right
*element,type=conn3d2,elset=conn_tie_rod_prevRigRot_right
*connector section, elset=conn_tie_rod_prevRigRot_right,behavior=conn_tie_rod_prevRigRot_right
join,cardan
conn_tie_rod_prevRigRot_right,
*connector behavior, name=conn_tie_rod_prevRigRot_right
*connector elasticity,comp=4
<conelPrevSteer>,
*connector elasticity,comp=5
<conelPrevSteer>,
*connector elasticity,comp=6
<conelPrevSteer>,
**--------------------------------------
*ORIENTATION,NAME=ori_rack_steering
*ELEMENT, TYPE=CONN3D2, ELSET=conn_rack_steering
*CONNECTOR SECTION, ELSET=conn_rack_steering
slot,align
ori_rack_steering,
*nset,nset=rack_and_pinion
**---------------------------------------
*elset,elset=conn_all
conn_steer_left,conn_steer_right,conn_rack_steering
**